ACR122U NFC Reader SDK: Driver Installation Guide

www.acs.com.hk

Introduction to PC/SC Driver

The ACS CCID Driver is a Microsoft WHQL-certified driver following the CCID Standard.

Driver Installation Procedure

A step by step guide to installing device drivers:

1. Insert the ACR122U NFC Reader SDK CD-ROM into your CD-ROM drive. If the screen below does not appear, run x:\ACR122USDK.EXE where x is the drive letter of your CD-ROM. |
2. Click on "Install ACS CCID Driver". |
3. Select the language of your choice and then click “OK”. |
4. Please wait while the Windows Installer prepares the installation. |
5. Click “Next” to continue with the installation. |
6. Choose Destination Location. Setup will install ACS CCID PCSC driver in the following folder x:\Program Files\ACR122U PCSC Driver 1.1.6.2\ where x is the driver letter of your local Windows drive. To install this folder, click “Next”. To install to a different folder, click “Browse” and select another folder then click “Next”.

7. Click “Install”. |
8. Wait for setup to be completed. |
9. Please plug in the reader then click on “Finish” to exit the program. |